

|  |  |  |  |
| --- | --- | --- | --- |
| **Technical Specification no. 230704**  **Tight Head Steel Drum TH 888** | | | |
|  | | Material | Cold rolled steel DC01 |
| Capacity | 216,5 dm³ |
| Construction | cylindrical body electrically welded, 2 rolling beads in the body plus additional Spiraltainer® corrugations; top and bottom connected with body by triple safety seaming SPIRALON® |
| Closures | original Tri-Sure® closures in the lid, 2’’ and ¾’’ with BN washers |
| **Gauges** | |
| Top | 0,8 mm |
| Body | 0,8 mm |
| Bottom | 0,8 mm |
| **UN** | |
| Bottom | UN 1A1/ Y1.5/ 150/\*/ 0,8-0,8-0,8 |
| Body | UN 1A1/ Y1.5/ 150/\*/NL/TCPI- GEFPL- 160583 |
| **Dimensions** | | **Finishing outside** | |
| Height | 880±3 mm | Top | Blue RAL5010 |
| External diameter | 595 mm | Body | Blue RAL5010 |
| Internal diameter | 571±2 mm | Bottom | Blue RAL5010 |
| Weight | 13,9 kg ± 1% | **Finishing inside** | |
|  | |
| Top | plain |
| Body | plain |
| Bottom | plain |
| Certified Management System: ISO 9001:2015, PN-EN 15593:2010 | | | |