

|  |
| --- |
| **Technical Specification no. 230503****Open Head Steel Drum OH 881 with removable lid, Internally coated with lacquer** |
|  | Material | Cold rolled steel DC01 |
| Capacity | 210 dm³ |
| Construction | cylindrical body, body seam electrically welded with 2 beads pressed out of the body, bottom made in Spiralon® technology. |
| Closures | removable lid with galvanised closing ring and rubber gasket Ø9,00 mm |
| **Gauges** |
| Lid | 0,8 mm |
| Body | 0,8 mm |
| Bottom | 1,0 mm |
| **UN Certificate** |
| Bottom | N/A |
| Body | N/A |
| **Dimensions** | **External coating** |
| Height | 880±3 mm | Lid | Blue colour RAL 5010 |
| Outside diameter | 595 mm | Body | Blue colour RAL 5010 |
| Inside diameter | 571±2 mm | Bottom | Blue colour RAL 5010 |
| Weight | approx. 14,9±1 % | **Internal lining** |
|  |
| Lid | Water‐based lacquer for food contact |
| Body |
| Bottom |
| **Certified Management System**  |
| PN‐EN 15593:2010 | PL014502 |
| ISO 9001:2015 | PL014502/P |